(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "Module_A20_2U" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 2.54 0))
    (property "Value" "Module_A20_2U" (id 1) (at 17.78 2.54 0))
    (property "Footprint" "Fabmicro:Module_A20" (id 2) (at 7.62 2.54 0))
    (property "Datasheet" "" (id 3) (at 7.62 2.54 0))
    (property "ki_locked" "" (id 4) (at 0 0 0))
    (symbol "Module_A20_2U_1_1"
      (pin output line (at -5.08 -10.16 0) (length 5.08)
        (name "CSI_VSYNC")
        (number "1")
      )
      (pin input line (at -5.08 -30.48 0) (length 5.08)
        (name "CSI_D7")
        (number "10")
      )
      (pin input line (at 35.56 -147.32 180) (length 5.08)
        (name "LRADC0")
        (number "100")
      )
      (pin input line (at 35.56 -149.86 180) (length 5.08)
        (name "LRADC1")
        (number "101")
      )
      (pin output line (at 35.56 -137.16 180) (length 5.08)
        (name "HPCOM")
        (number "102")
      )
      (pin output line (at 35.56 -142.24 180) (length 5.08)
        (name "AOUT_R")
        (number "103")
      )
      (pin output line (at 35.56 -139.7 180) (length 5.08)
        (name "AOUT_L")
        (number "104")
      )
      (pin bidirectional line (at 35.56 -111.76 180) (length 5.08)
        (name "USB2_N")
        (number "105")
      )
      (pin bidirectional line (at 35.56 -114.3 180) (length 5.08)
        (name "USB2_P")
        (number "106")
      )
      (pin bidirectional line (at 35.56 -106.68 180) (length 5.08)
        (name "USB1_N")
        (number "107")
      )
      (pin bidirectional line (at 35.56 -109.22 180) (length 5.08)
        (name "USB1_P")
        (number "108")
      )
      (pin bidirectional line (at 35.56 -101.6 180) (length 5.08)
        (name "USB0_N")
        (number "109")
      )
      (pin input line (at 35.56 -76.2 180) (length 5.08)
        (name "LCD_PWM")
        (number "11")
      )
      (pin bidirectional line (at 35.56 -104.14 180) (length 5.08)
        (name "USB0_P")
        (number "110")
      )
      (pin bidirectional line (at -5.08 -86.36 0) (length 5.08)
        (name "SDCO_D0")
        (number "111")
      )
      (pin bidirectional line (at -5.08 -88.9 0) (length 5.08)
        (name "SDCO_D1")
        (number "112")
      )
      (pin bidirectional line (at -5.08 -91.44 0) (length 5.08)
        (name "SDCO_D2")
        (number "113")
      )
      (pin bidirectional line (at -5.08 -93.98 0) (length 5.08)
        (name "SDCO_D3")
        (number "114")
      )
      (pin input line (at -5.08 -96.52 0) (length 5.08)
        (name "SDCO_CMD")
        (number "115")
      )
      (pin output line (at -5.08 -99.06 0) (length 5.08)
        (name "SDCO_CLK")
        (number "116")
      )
      (pin input line (at -5.08 -101.6 0) (length 5.08)
        (name "SDC0_DET")
        (number "117")
      )
      (pin output line (at -5.08 -5.08 0) (length 5.08)
        (name "CSI_MCLK")
        (number "118")
      )
      (pin output line (at -5.08 -2.54 0) (length 5.08)
        (name "CSI_PCLK")
        (number "119")
      )
      (pin input line (at -5.08 -114.3 0) (length 5.08)
        (name "UART5_RX")
        (number "12")
      )
      (pin output line (at 35.56 -93.98 180) (length 5.08)
        (name "EXTEN")
        (number "122")
      )
      (pin input line (at 35.56 -160.02 180) (length 5.08)
        (name "USB0_DRV")
        (number "124")
      )
      (pin output line (at -5.08 -111.76 0) (length 5.08)
        (name "UART5_TX")
        (number "13")
      )
      (pin input line (at 35.56 -157.48 180) (length 5.08)
        (name "RESET_N")
        (number "19")
      )
      (pin output line (at -5.08 -7.62 0) (length 5.08)
        (name "CSI_HSYNC")
        (number "2")
      )
      (pin output line (at -5.08 -116.84 0) (length 5.08)
        (name "UART6_TX")
        (number "20")
      )
      (pin input line (at -5.08 -119.38 0) (length 5.08)
        (name "UART6_RX")
        (number "21")
      )
      (pin bidirectional line (at -5.08 -127 0) (length 5.08)
        (name "I2C0_SDA")
        (number "22")
      )
      (pin output line (at -5.08 -124.46 0) (length 5.08)
        (name "I2C0_SCK")
        (number "23")
      )
      (pin bidirectional line (at -5.08 -132.08 0) (length 5.08)
        (name "I2C1_SDA")
        (number "24")
      )
      (pin output line (at -5.08 -129.54 0) (length 5.08)
        (name "I2C1_SCK")
        (number "25")
      )
      (pin bidirectional line (at -5.08 -137.16 0) (length 5.08)
        (name "I2C2_SDA")
        (number "26")
      )
      (pin output line (at -5.08 -134.62 0) (length 5.08)
        (name "I2C2_SCK")
        (number "27")
      )
      (pin output line (at -5.08 -106.68 0) (length 5.08)
        (name "UART0_TX")
        (number "28")
      )
      (pin input line (at -5.08 -109.22 0) (length 5.08)
        (name "UART0_RX")
        (number "29")
      )
      (pin input line (at -5.08 -12.7 0) (length 5.08)
        (name "CSI_D0")
        (number "3")
      )
      (pin input line (at 35.56 -119.38 180) (length 5.08)
        (name "USB0_IDDET")
        (number "30")
      )
      (pin input line (at 35.56 -121.92 180) (length 5.08)
        (name "USB0_VBUSDET")
        (number "31")
      )
      (pin input line (at -5.08 -142.24 0) (length 5.08)
        (name "GPIO1")
        (number "32")
      )
      (pin input line (at -5.08 -144.78 0) (length 5.08)
        (name "GPIO2")
        (number "34")
      )
      (pin input line (at -5.08 -147.32 0) (length 5.08)
        (name "GPIO3")
        (number "35")
      )
      (pin input line (at -5.08 -149.86 0) (length 5.08)
        (name "GPIO4")
        (number "36")
      )
      (pin output line (at -5.08 -152.4 0) (length 5.08)
        (name "GPIO5")
        (number "37")
      )
      (pin output line (at -5.08 -154.94 0) (length 5.08)
        (name "GPIO6")
        (number "38")
      )
      (pin output line (at -5.08 -157.48 0) (length 5.08)
        (name "GPIO7")
        (number "39")
      )
      (pin input line (at -5.08 -15.24 0) (length 5.08)
        (name "CSI_D1")
        (number "4")
      )
      (pin output line (at -5.08 -160.02 0) (length 5.08)
        (name "GPIO8")
        (number "40")
      )
      (pin output line (at -5.08 -76.2 0) (length 5.08)
        (name "LAN_COL")
        (number "41")
      )
      (pin output line (at -5.08 -78.74 0) (length 5.08)
        (name "LAN_nINT")
        (number "42")
      )
      (pin output line (at -5.08 -73.66 0) (length 5.08)
        (name "LAN_CRS")
        (number "43")
      )
      (pin output line (at -5.08 -71.12 0) (length 5.08)
        (name "LAN_TXCLK")
        (number "44")
      )
      (pin output line (at -5.08 -68.58 0) (length 5.08)
        (name "LAN_TXEN")
        (number "45")
      )
      (pin input line (at -5.08 -66.04 0) (length 5.08)
        (name "LAN_MDIO")
        (number "46")
      )
      (pin input line (at -5.08 -63.5 0) (length 5.08)
        (name "LAN_MDC")
        (number "47")
      )
      (pin input line (at -5.08 -60.96 0) (length 5.08)
        (name "LAN_RXDV")
        (number "48")
      )
      (pin input line (at -5.08 -58.42 0) (length 5.08)
        (name "LAN_RXER")
        (number "49")
      )
      (pin input line (at -5.08 -17.78 0) (length 5.08)
        (name "CSI_D2")
        (number "5")
      )
      (pin input line (at -5.08 -55.88 0) (length 5.08)
        (name "LAN_RCLK")
        (number "50")
      )
      (pin output line (at -5.08 -45.72 0) (length 5.08)
        (name "LAN_TXD0")
        (number "51")
      )
      (pin output line (at -5.08 -48.26 0) (length 5.08)
        (name "LAN_TXD1")
        (number "52")
      )
      (pin output line (at -5.08 -50.8 0) (length 5.08)
        (name "LAN_TXD2")
        (number "53")
      )
      (pin output line (at -5.08 -53.34 0) (length 5.08)
        (name "LAN_TXD3")
        (number "54")
      )
      (pin input line (at -5.08 -35.56 0) (length 5.08)
        (name "LAN_RXD0")
        (number "55")
      )
      (pin input line (at -5.08 -38.1 0) (length 5.08)
        (name "LAN_RXD1")
        (number "56")
      )
      (pin input line (at -5.08 -40.64 0) (length 5.08)
        (name "LAN_RXD2")
        (number "57")
      )
      (pin input line (at -5.08 -43.18 0) (length 5.08)
        (name "LAN_RXD3")
        (number "58")
      )
      (pin output line (at -5.08 -81.28 0) (length 5.08)
        (name "LAN_nRST")
        (number "59")
      )
      (pin input line (at -5.08 -20.32 0) (length 5.08)
        (name "CSI_D3")
        (number "6")
      )
      (pin power_out line (at 35.56 -154.94 180) (length 5.08)
        (name "+3V3_IOVCC")
        (number "61")
      )
      (pin input line (at 35.56 -73.66 180) (length 5.08)
        (name "LCD_INT")
        (number "62")
      )
      (pin input line (at 35.56 -71.12 180) (length 5.08)
        (name "LCD_DE")
        (number "63")
      )
      (pin input line (at 35.56 -68.58 180) (length 5.08)
        (name "LCD_VSYNC")
        (number "64")
      )
      (pin input line (at 35.56 -66.04 180) (length 5.08)
        (name "LCD_HSYNC")
        (number "65")
      )
      (pin input line (at 35.56 -63.5 180) (length 5.08)
        (name "LCD_CLK")
        (number "66")
      )
      (pin input line (at 35.56 -60.96 180) (length 5.08)
        (name "LCD_D23")
        (number "67")
      )
      (pin input line (at 35.56 -58.42 180) (length 5.08)
        (name "LCD_D22")
        (number "68")
      )
      (pin input line (at 35.56 -55.88 180) (length 5.08)
        (name "LCD_D21")
        (number "69")
      )
      (pin input line (at -5.08 -22.86 0) (length 5.08)
        (name "CSI_D4")
        (number "7")
      )
      (pin input line (at 35.56 -53.34 180) (length 5.08)
        (name "LCD_D20")
        (number "70")
      )
      (pin input line (at 35.56 -50.8 180) (length 5.08)
        (name "LCD_D19")
        (number "71")
      )
      (pin input line (at 35.56 -48.26 180) (length 5.08)
        (name "LCD_D18")
        (number "72")
      )
      (pin input line (at 35.56 -45.72 180) (length 5.08)
        (name "LCD_D17")
        (number "73")
      )
      (pin input line (at 35.56 -43.18 180) (length 5.08)
        (name "LCD_D16")
        (number "74")
      )
      (pin input line (at 35.56 -40.64 180) (length 5.08)
        (name "LCD_D15")
        (number "75")
      )
      (pin input line (at 35.56 -38.1 180) (length 5.08)
        (name "LCD_D14")
        (number "76")
      )
      (pin input line (at 35.56 -35.56 180) (length 5.08)
        (name "LCD_D13")
        (number "77")
      )
      (pin input line (at 35.56 -33.02 180) (length 5.08)
        (name "LCD_D12")
        (number "78")
      )
      (pin input line (at 35.56 -30.48 180) (length 5.08)
        (name "LCD_D11")
        (number "79")
      )
      (pin input line (at -5.08 -25.4 0) (length 5.08)
        (name "CSI_D5")
        (number "8")
      )
      (pin input line (at 35.56 -27.94 180) (length 5.08)
        (name "LCD_D10")
        (number "80")
      )
      (pin input line (at 35.56 -25.4 180) (length 5.08)
        (name "LCD_D9")
        (number "81")
      )
      (pin input line (at 35.56 -22.86 180) (length 5.08)
        (name "LCD_D8")
        (number "82")
      )
      (pin input line (at 35.56 -20.32 180) (length 5.08)
        (name "LCD_D7")
        (number "83")
      )
      (pin input line (at 35.56 -17.78 180) (length 5.08)
        (name "LCD_D6")
        (number "84")
      )
      (pin input line (at 35.56 -15.24 180) (length 5.08)
        (name "LCD_D5")
        (number "85")
      )
      (pin input line (at 35.56 -12.7 180) (length 5.08)
        (name "LCD_D4")
        (number "86")
      )
      (pin input line (at 35.56 -10.16 180) (length 5.08)
        (name "LCD_D3")
        (number "87")
      )
      (pin input line (at 35.56 -7.62 180) (length 5.08)
        (name "LCD_D2")
        (number "88")
      )
      (pin input line (at 35.56 -5.08 180) (length 5.08)
        (name "LCD_D1")
        (number "89")
      )
      (pin input line (at -5.08 -27.94 0) (length 5.08)
        (name "CSI_D6")
        (number "9")
      )
      (pin input line (at 35.56 -2.54 180) (length 5.08)
        (name "LCD_D0")
        (number "90")
      )
      (pin output line (at 35.56 -96.52 180) (length 5.08)
        (name "CVBS_OUT")
        (number "91")
      )
      (pin input line (at 35.56 -86.36 180) (length 5.08)
        (name "TPX2")
        (number "92")
      )
      (pin input line (at 35.56 -81.28 180) (length 5.08)
        (name "TPX1")
        (number "94")
      )
      (pin input line (at 35.56 -88.9 180) (length 5.08)
        (name "TPY2")
        (number "95")
      )
      (pin input line (at 35.56 -83.82 180) (length 5.08)
        (name "TPY1")
        (number "96")
      )
      (pin input line (at 35.56 -129.54 180) (length 5.08)
        (name "MIC1_IN")
        (number "97")
      )
      (pin input line (at 35.56 -132.08 180) (length 5.08)
        (name "MIC2_IN")
        (number "98")
      )
      (pin output line (at 35.56 -127 180) (length 5.08)
        (name "VMIC")
        (number "99")
      )
    )
    (symbol "Module_A20_2U_2_1"
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "GND")
        (number "120")
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "GND")
        (number "121")
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "GND")
        (number "123")
      )
      (pin power_in line (at -5.08 -17.78 0) (length 5.08)
        (name "GND")
        (number "125")
      )
      (pin power_in line (at -5.08 -20.32 0) (length 5.08)
        (name "GND")
        (number "126")
      )
      (pin power_in line (at -5.08 -22.86 0) (length 5.08)
        (name "GND")
        (number "127")
      )
      (pin power_in line (at -5.08 -25.4 0) (length 5.08)
        (name "GND")
        (number "128")
      )
      (pin power_in line (at -5.08 -35.56 0) (length 5.08)
        (name "GND")
        (number "129")
      )
      (pin power_in line (at -5.08 -33.02 0) (length 5.08)
        (name "GND")
        (number "130")
      )
      (pin power_in line (at -5.08 -30.48 0) (length 5.08)
        (name "GND")
        (number "131")
      )
      (pin power_in line (at -5.08 -27.94 0) (length 5.08)
        (name "GND")
        (number "132")
      )
      (pin power_in line (at -5.08 -45.72 0) (length 5.08)
        (name "GND")
        (number "133")
      )
      (pin power_in line (at -5.08 -43.18 0) (length 5.08)
        (name "GND")
        (number "134")
      )
      (pin power_in line (at -5.08 -40.64 0) (length 5.08)
        (name "GND")
        (number "135")
      )
      (pin power_in line (at -5.08 -38.1 0) (length 5.08)
        (name "GND")
        (number "136")
      )
      (pin power_in line (at -5.08 -48.26 0) (length 5.08)
        (name "GND")
        (number "137")
      )
      (pin power_in line (at -5.08 -50.8 0) (length 5.08)
        (name "GND")
        (number "138")
      )
      (pin power_in line (at -5.08 -53.34 0) (length 5.08)
        (name "GND")
        (number "139")
      )
      (pin power_in line (at 35.56 -12.7 180) (length 5.08)
        (name "+5V0_IN")
        (number "14")
      )
      (pin power_in line (at -5.08 -55.88 0) (length 5.08)
        (name "GND")
        (number "140")
      )
      (pin power_in line (at -5.08 -58.42 0) (length 5.08)
        (name "GND")
        (number "141")
      )
      (pin power_in line (at -5.08 -60.96 0) (length 5.08)
        (name "GND")
        (number "142")
      )
      (pin power_in line (at -5.08 -63.5 0) (length 5.08)
        (name "GND")
        (number "143")
      )
      (pin power_in line (at -5.08 -66.04 0) (length 5.08)
        (name "GND")
        (number "144")
      )
      (pin power_in line (at -5.08 -68.58 0) (length 5.08)
        (name "GND")
        (number "145")
      )
      (pin power_in line (at -5.08 -71.12 0) (length 5.08)
        (name "GND")
        (number "146")
      )
      (pin power_in line (at -5.08 -73.66 0) (length 5.08)
        (name "GND")
        (number "147")
      )
      (pin power_in line (at -5.08 -76.2 0) (length 5.08)
        (name "GND")
        (number "148")
      )
      (pin power_in line (at -5.08 -78.74 0) (length 5.08)
        (name "GND")
        (number "149")
      )
      (pin power_in line (at 35.56 -10.16 180) (length 5.08)
        (name "+5V0_IN")
        (number "15")
      )
      (pin power_in line (at -5.08 -81.28 0) (length 5.08)
        (name "GND")
        (number "150")
      )
      (pin power_in line (at -5.08 -83.82 0) (length 5.08)
        (name "GND")
        (number "151")
      )
      (pin power_in line (at -5.08 -86.36 0) (length 5.08)
        (name "GND")
        (number "152")
      )
      (pin power_in line (at -5.08 -88.9 0) (length 5.08)
        (name "GND")
        (number "153")
      )
      (pin power_in line (at -5.08 -91.44 0) (length 5.08)
        (name "GND")
        (number "154")
      )
      (pin power_in line (at -5.08 -93.98 0) (length 5.08)
        (name "GND")
        (number "155")
      )
      (pin power_in line (at -5.08 -96.52 0) (length 5.08)
        (name "GND")
        (number "156")
      )
      (pin power_in line (at -5.08 -99.06 0) (length 5.08)
        (name "GND")
        (number "157")
      )
      (pin power_in line (at -5.08 -101.6 0) (length 5.08)
        (name "GND")
        (number "158")
      )
      (pin power_in line (at -5.08 -104.14 0) (length 5.08)
        (name "GND")
        (number "159")
      )
      (pin power_in line (at 35.56 -7.62 180) (length 5.08)
        (name "VBUS")
        (number "16")
      )
      (pin power_in line (at -5.08 -106.68 0) (length 5.08)
        (name "GND")
        (number "160")
      )
      (pin power_in line (at -5.08 -109.22 0) (length 5.08)
        (name "GND")
        (number "161")
      )
      (pin power_in line (at -5.08 -111.76 0) (length 5.08)
        (name "GND")
        (number "162")
      )
      (pin power_in line (at -5.08 -114.3 0) (length 5.08)
        (name "GND")
        (number "163")
      )
      (pin power_in line (at -5.08 -116.84 0) (length 5.08)
        (name "GND")
        (number "164")
      )
      (pin power_in line (at -5.08 -119.38 0) (length 5.08)
        (name "GND")
        (number "165")
      )
      (pin power_in line (at -5.08 -121.92 0) (length 5.08)
        (name "GND")
        (number "166")
      )
      (pin power_in line (at -5.08 -124.46 0) (length 5.08)
        (name "x")
        (number "167")
      )
      (pin power_in line (at -5.08 -127 0) (length 5.08)
        (name "GND")
        (number "168")
      )
      (pin power_in line (at 35.56 -5.08 180) (length 5.08)
        (name "AXP209_BACKUP")
        (number "17")
      )
      (pin power_out line (at 35.56 -2.54 180) (length 5.08)
        (name "IPSOUT")
        (number "18")
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "GND")
        (number "33")
      )
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "GND")
        (number "60")
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "GND")
        (number "93")
      )
    )
  )
)
