(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "RanetkaPC_Module" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 2.54 0))
    (property "Value" "RanetkaPC_Module" (id 1) (at 17.78 2.54 0))
    (property "Footprint" "RanetkaPC_Module:RanetkaPC_Module" (id 2) (at 20.32 -215.9 0))
    (property "Datasheet" "" (id 3) (at 7.62 2.54 0))
    (property "Mfr. Part Number" "RanetkaPC_Module_V1" (id 4) (at 38.1 -215.9 0))
    (property "ki_locked" "" (id 5) (at 0 0 0))
    (symbol "RanetkaPC_Module_1_1"
      (pin input line (at -5.08 -43.18 0) (length 5.08)
        (name "MIPI_CSI_RX_CLK_P")
        (number "1")
      )
      (pin input line (at -5.08 -63.5 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA0_P")
        (number "10")
      )
      (pin input line (at 50.8 -154.94 180) (length 5.08)
        (name "LRADC0")
        (number "100")
      )
      (pin input line (at 50.8 -157.48 180) (length 5.08)
        (name "LRADC1")
        (number "101")
      )
      (pin output line (at 50.8 -144.78 180) (length 5.08)
        (name "HPCOM")
        (number "102")
      )
      (pin output line (at 50.8 -147.32 180) (length 5.08)
        (name "HPR_OUT")
        (number "103")
      )
      (pin output line (at 50.8 -149.86 180) (length 5.08)
        (name "HPL_OUT")
        (number "104")
      )
      (pin bidirectional line (at 50.8 -127 180) (length 5.08)
        (name "UDM1_N")
        (number "105")
      )
      (pin bidirectional line (at 50.8 -129.54 180) (length 5.08)
        (name "UDP1_P")
        (number "106")
      )
      (pin bidirectional line (at 50.8 -162.56 180) (length 5.08)
        (name "CAN0_TX")
        (number "107")
      )
      (pin bidirectional line (at 50.8 -165.1 180) (length 5.08)
        (name "CAN0_RX")
        (number "108")
      )
      (pin bidirectional line (at 50.8 -121.92 180) (length 5.08)
        (name "UDM0_N")
        (number "109")
      )
      (pin input line (at 50.8 -76.2 180) (length 5.08)
        (name "LCD_PWM")
        (number "11")
      )
      (pin bidirectional line (at 50.8 -124.46 180) (length 5.08)
        (name "UDP0_P")
        (number "110")
      )
      (pin bidirectional line (at -5.08 -68.58 0) (length 5.08)
        (name "SDCO_D0")
        (number "111")
      )
      (pin bidirectional line (at -5.08 -71.12 0) (length 5.08)
        (name "SDCO_D1")
        (number "112")
      )
      (pin bidirectional line (at -5.08 -73.66 0) (length 5.08)
        (name "SDCO_D2")
        (number "113")
      )
      (pin bidirectional line (at -5.08 -76.2 0) (length 5.08)
        (name "SDCO_D3")
        (number "114")
      )
      (pin input line (at -5.08 -78.74 0) (length 5.08)
        (name "SDCO_CMD")
        (number "115")
      )
      (pin output line (at -5.08 -81.28 0) (length 5.08)
        (name "SDCO_CLK")
        (number "116")
      )
      (pin input line (at -5.08 -83.82 0) (length 5.08)
        (name "SDC0_DET")
        (number "117")
      )
      (pin output line (at -5.08 -35.56 0) (length 5.08)
        (name "MIPI_CSI_CLK")
        (number "118")
      )
      (pin output line (at -5.08 -38.1 0) (length 5.08)
        (name "MIPI_CSI_FSYNC")
        (number "119")
      )
      (pin input line (at -5.08 -88.9 0) (length 5.08)
        (name "UART2_RX")
        (number "12")
      )
      (pin output line (at 50.8 -208.28 180) (length 5.08)
        (name "EXTEN")
        (number "122")
      )
      (pin output line (at -5.08 -198.12 0) (length 5.08)
        (name "PCI0_PERSTN")
        (number "123")
      )
      (pin input line (at 50.8 -175.26 180) (length 5.08)
        (name "USB0_DRV")
        (number "124")
      )
      (pin input line (at -5.08 -200.66 0) (length 5.08)
        (name "PCI0_WAKE")
        (number "125")
      )
      (pin input line (at -5.08 -203.2 0) (length 5.08)
        (name "PCI0_APP")
        (number "126")
      )
      (pin input line (at -5.08 -195.58 0) (length 5.08)
        (name "PCI0_CLKREQ")
        (number "127")
      )
      (pin input line (at -5.08 -205.74 0) (length 5.08)
        (name "PCI0_PHY")
        (number "128")
      )
      (pin output line (at -5.08 -182.88 0) (length 5.08)
        (name "PCI0_TX0P")
        (number "129")
      )
      (pin output line (at -5.08 -91.44 0) (length 5.08)
        (name "UART2_TX")
        (number "13")
      )
      (pin output line (at -5.08 -180.34 0) (length 5.08)
        (name "PCI0_TX0N")
        (number "130")
      )
      (pin output line (at -5.08 -187.96 0) (length 5.08)
        (name "PCI0_TX1P")
        (number "132")
      )
      (pin output line (at -5.08 -185.42 0) (length 5.08)
        (name "PCI0_TX1N")
        (number "133")
      )
      (pin input line (at -5.08 -177.8 0) (length 5.08)
        (name "PCI0_RX1P")
        (number "135")
      )
      (pin input line (at -5.08 -175.26 0) (length 5.08)
        (name "PCI0_RX1N")
        (number "136")
      )
      (pin input line (at -5.08 -170.18 0) (length 5.08)
        (name "PCI0_RX0N")
        (number "138")
      )
      (pin input line (at -5.08 -172.72 0) (length 5.08)
        (name "PCI0_RX0P")
        (number "139")
      )
      (pin output line (at -5.08 -190.5 0) (length 5.08)
        (name "PCI0_CLKN")
        (number "141")
      )
      (pin output line (at -5.08 -193.04 0) (length 5.08)
        (name "PCI0_CLKP")
        (number "142")
      )
      (pin input line (at 50.8 -195.58 180) (length 5.08)
        (name "JESD_SYNCB_0")
        (number "147")
      )
      (pin input line (at 50.8 -180.34 180) (length 5.08)
        (name "JESD0_CLKX")
        (number "148")
      )
      (pin input line (at 50.8 -182.88 180) (length 5.08)
        (name "JESD0_CKL")
        (number "149")
      )
      (pin output line (at 50.8 -185.42 180) (length 5.08)
        (name "JESD0_SYSREF")
        (number "150")
      )
      (pin output line (at 50.8 -187.96 180) (length 5.08)
        (name "JESD0_SYSREFX")
        (number "151")
      )
      (pin output line (at 50.8 -198.12 180) (length 5.08)
        (name "JESD_SYNCB_0X")
        (number "152")
      )
      (pin input line (at 50.8 -190.5 180) (length 5.08)
        (name "SPARE_LVDS_RX")
        (number "153")
      )
      (pin input line (at 50.8 -193.04 180) (length 5.08)
        (name "SPARE_LVDS_RXX")
        (number "154")
      )
      (pin output line (at 50.8 -111.76 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA2_P")
        (number "157")
      )
      (pin output line (at 50.8 -109.22 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA2_N")
        (number "158")
      )
      (pin output line (at 50.8 -116.84 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA3_P")
        (number "159")
      )
      (pin output line (at 50.8 -114.3 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA3_N")
        (number "160")
      )
      (pin output line (at -5.08 -165.1 0) (length 5.08)
        (name "CLK125")
        (number "161")
      )
      (pin output line (at 50.8 -99.06 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA0_N")
        (number "162")
      )
      (pin output line (at 50.8 -101.6 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA0_P")
        (number "163")
      )
      (pin output line (at 50.8 -106.68 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA1_P")
        (number "164")
      )
      (pin output line (at 50.8 -104.14 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA1_N")
        (number "165")
      )
      (pin output line (at 50.8 -93.98 180) (length 5.08)
        (name "MIPI_DSI_TX_CLK_N")
        (number "166")
      )
      (pin output line (at 50.8 -96.52 180) (length 5.08)
        (name "MIPI_DSI_TX_CLK_P")
        (number "167")
      )
      (pin input line (at 50.8 -205.74 180) (length 5.08)
        (name "PWRGD_RST")
        (number "19")
      )
      (pin input line (at -5.08 -40.64 0) (length 5.08)
        (name "MIPI_CSI_RX_CLK_N")
        (number "2")
      )
      (pin output line (at -5.08 -93.98 0) (length 5.08)
        (name "UART1_TX")
        (number "20")
      )
      (pin input line (at -5.08 -96.52 0) (length 5.08)
        (name "UART1_RX")
        (number "21")
      )
      (pin bidirectional line (at -5.08 -106.68 0) (length 5.08)
        (name "I2C3_SDA/I2C0_SDA")
        (number "22")
      )
      (pin output line (at -5.08 -109.22 0) (length 5.08)
        (name "I2C3_SCK/I2C0_SCK")
        (number "23")
      )
      (pin bidirectional line (at -5.08 -111.76 0) (length 5.08)
        (name "I2C1_SDA")
        (number "24")
      )
      (pin output line (at -5.08 -114.3 0) (length 5.08)
        (name "I2C1_SCK")
        (number "25")
      )
      (pin bidirectional line (at -5.08 -116.84 0) (length 5.08)
        (name "I2C2_SDA")
        (number "26")
      )
      (pin output line (at -5.08 -119.38 0) (length 5.08)
        (name "I2C2_SCK")
        (number "27")
      )
      (pin output line (at -5.08 -99.06 0) (length 5.08)
        (name "UART0_TX")
        (number "28")
      )
      (pin input line (at -5.08 -101.6 0) (length 5.08)
        (name "UART0_RX")
        (number "29")
      )
      (pin input line (at -5.08 -45.72 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA3_P")
        (number "3")
      )
      (pin input line (at 50.8 -170.18 180) (length 5.08)
        (name "USB0_IDDET")
        (number "30")
      )
      (pin input line (at 50.8 -172.72 180) (length 5.08)
        (name "USB0_VBUSDET")
        (number "31")
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "GPIO1")
        (number "32")
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "GPIO2")
        (number "34")
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "GPIO3")
        (number "35")
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "GPIO4")
        (number "36")
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "GPIO5")
        (number "37")
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "GPIO6")
        (number "38")
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "GPIO7")
        (number "39")
      )
      (pin input line (at -5.08 -48.26 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA3_N")
        (number "4")
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "GPIO8")
        (number "40")
      )
      (pin bidirectional line (at -5.08 -30.4801 0) (length 5.08)
        (name "GPIO12/RMII0_COL")
        (number "41")
      )
      (pin bidirectional line (at -5.08 -160.02 0) (length 5.08)
        (name "RGMII0_nINT/RMII0_nINT")
        (number "42")
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "GPIO11/RMII0_CRS")
        (number "43")
      )
      (pin bidirectional line (at -5.08 -157.48 0) (length 5.08)
        (name "RGMII0_TXC/RMII0_TXCLK")
        (number "44")
      )
      (pin bidirectional line (at -5.08 -154.94 0) (length 5.08)
        (name "RGMII0_TXCTL/RMII0_TXEN")
        (number "45")
      )
      (pin bidirectional line (at -5.08 -147.32 0) (length 5.08)
        (name "RGMII0_MDIO/RMII0_MDIO")
        (number "46")
      )
      (pin input line (at -5.08 -144.78 0) (length 5.08)
        (name "RGMII0_MDC/RMII0_MDC")
        (number "47")
      )
      (pin input line (at -5.08 -149.86 0) (length 5.08)
        (name "RGMII0_RXCTL/RMII0_RXDV")
        (number "48")
      )
      (pin output line (at -5.08 -25.4 0) (length 5.08)
        (name "GPIO10/RMII0_RXER")
        (number "49")
      )
      (pin input line (at -5.08 -50.8 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA2_N")
        (number "5")
      )
      (pin input line (at -5.08 -152.4 0) (length 5.08)
        (name "RGMII0_RXC/RMII0_RCLK")
        (number "50")
      )
      (pin output line (at -5.08 -142.24 0) (length 5.08)
        (name "RGMII0_TXD0/RMII0_TXD0")
        (number "51")
      )
      (pin output line (at -5.08 -139.7 0) (length 5.08)
        (name "RGMII0_TXD1/RMII0_TXD1")
        (number "52")
      )
      (pin output line (at -5.08 -137.16 0) (length 5.08)
        (name "RGMII0_TXD2/RMII0_TXD2")
        (number "53")
      )
      (pin output line (at -5.08 -134.62 0) (length 5.08)
        (name "RGMII0_TXD3/RMII0_TXD3")
        (number "54")
      )
      (pin input line (at -5.08 -132.08 0) (length 5.08)
        (name "RGMII0_RXD0/RMII0_RXD0")
        (number "55")
      )
      (pin input line (at -5.08 -129.54 0) (length 5.08)
        (name "RGMII0_RXD1/RMII0_RXD1")
        (number "56")
      )
      (pin input line (at -5.08 -127 0) (length 5.08)
        (name "RGMII0_RXD2/RMII0_RXD2")
        (number "57")
      )
      (pin input line (at -5.08 -124.46 0) (length 5.08)
        (name "RGMII0_RXD3/RMII0_RXD3")
        (number "58")
      )
      (pin output line (at -5.08 -162.56 0) (length 5.08)
        (name "RGMII0_nRST/RMII0_nRST")
        (number "59")
      )
      (pin input line (at -5.08 -53.34 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA2_P")
        (number "6")
      )
      (pin power_out line (at 50.8 -203.2 180) (length 5.08)
        (name "+3V3_IOVCC")
        (number "61")
      )
      (pin input line (at 50.8 -73.66 180) (length 5.08)
        (name "TCP_INT")
        (number "62")
      )
      (pin input line (at 50.8 -71.12 180) (length 5.08)
        (name "LCD_DE")
        (number "63")
      )
      (pin input line (at 50.8 -68.58 180) (length 5.08)
        (name "LCD_VSYNC")
        (number "64")
      )
      (pin input line (at 50.8 -66.04 180) (length 5.08)
        (name "LCD_HSYNC")
        (number "65")
      )
      (pin input line (at 50.8 -63.5 180) (length 5.08)
        (name "LCD_CLK")
        (number "66")
      )
      (pin input line (at 50.8 -60.96 180) (length 5.08)
        (name "LCD_D23")
        (number "67")
      )
      (pin input line (at 50.8 -58.42 180) (length 5.08)
        (name "LCD_D22")
        (number "68")
      )
      (pin input line (at 50.8 -55.88 180) (length 5.08)
        (name "LCD_D21")
        (number "69")
      )
      (pin input line (at -5.08 -55.88 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA1_P")
        (number "7")
      )
      (pin input line (at 50.8 -53.34 180) (length 5.08)
        (name "LCD_D20")
        (number "70")
      )
      (pin input line (at 50.8 -50.8 180) (length 5.08)
        (name "LCD_D19")
        (number "71")
      )
      (pin input line (at 50.8 -48.26 180) (length 5.08)
        (name "LCD_D18")
        (number "72")
      )
      (pin input line (at 50.8 -45.72 180) (length 5.08)
        (name "LCD_D17")
        (number "73")
      )
      (pin input line (at 50.8 -43.18 180) (length 5.08)
        (name "LCD_D16")
        (number "74")
      )
      (pin input line (at 50.8 -40.64 180) (length 5.08)
        (name "LCD_D15")
        (number "75")
      )
      (pin input line (at 50.8 -38.1 180) (length 5.08)
        (name "LCD_D14")
        (number "76")
      )
      (pin input line (at 50.8 -35.56 180) (length 5.08)
        (name "LCD_D13")
        (number "77")
      )
      (pin input line (at 50.8 -33.02 180) (length 5.08)
        (name "LCD_D12")
        (number "78")
      )
      (pin input line (at 50.8 -30.48 180) (length 5.08)
        (name "LCD_D11")
        (number "79")
      )
      (pin input line (at -5.08 -58.42 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA1_N")
        (number "8")
      )
      (pin input line (at 50.8 -27.94 180) (length 5.08)
        (name "LCD_D10")
        (number "80")
      )
      (pin input line (at 50.8 -25.4 180) (length 5.08)
        (name "LCD_D9")
        (number "81")
      )
      (pin input line (at 50.8 -22.86 180) (length 5.08)
        (name "LCD_D8")
        (number "82")
      )
      (pin input line (at 50.8 -20.32 180) (length 5.08)
        (name "LCD_D7")
        (number "83")
      )
      (pin input line (at 50.8 -17.78 180) (length 5.08)
        (name "LCD_D6")
        (number "84")
      )
      (pin input line (at 50.8 -15.24 180) (length 5.08)
        (name "LCD_D5")
        (number "85")
      )
      (pin input line (at 50.8 -12.7 180) (length 5.08)
        (name "LCD_D4")
        (number "86")
      )
      (pin input line (at 50.8 -10.16 180) (length 5.08)
        (name "LCD_D3")
        (number "87")
      )
      (pin input line (at 50.8 -7.62 180) (length 5.08)
        (name "LCD_D2")
        (number "88")
      )
      (pin input line (at 50.8 -5.08 180) (length 5.08)
        (name "LCD_D1")
        (number "89")
      )
      (pin input line (at -5.08 -60.96 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA0_N")
        (number "9")
      )
      (pin input line (at 50.8 -2.54 180) (length 5.08)
        (name "LCD_D0")
        (number "90")
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "GPIO9")
        (number "91")
      )
      (pin input line (at 50.8 -86.36 180) (length 5.08)
        (name "TPX2")
        (number "92")
      )
      (pin input line (at 50.8 -81.28 180) (length 5.08)
        (name "TPX1")
        (number "94")
      )
      (pin input line (at 50.8 -88.9 180) (length 5.08)
        (name "TPY2")
        (number "95")
      )
      (pin input line (at 50.8 -83.82 180) (length 5.08)
        (name "TPY1")
        (number "96")
      )
      (pin input line (at 50.8 -137.16 180) (length 5.08)
        (name "MIC1_IN")
        (number "97")
      )
      (pin input line (at 50.8 -139.7 180) (length 5.08)
        (name "MIC2_IN")
        (number "98")
      )
      (pin output line (at 50.8 -134.62 180) (length 5.08)
        (name "VMIC")
        (number "99")
      )
    )
    (symbol "RanetkaPC_Module_2_1"
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "GND")
        (number "120")
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "GND")
        (number "121")
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "GND")
        (number "131")
      )
      (pin power_in line (at -5.08 -17.78 0) (length 5.08)
        (name "GND")
        (number "134")
      )
      (pin power_in line (at -5.08 -20.32 0) (length 5.08)
        (name "GND")
        (number "137")
      )
      (pin power_in line (at 50.8 -15.24 180) (length 5.08)
        (name "+5V0_IN")
        (number "14")
      )
      (pin power_in line (at -5.08 -22.86 0) (length 5.08)
        (name "GND")
        (number "140")
      )
      (pin power_in line (at -5.08 -25.4 0) (length 5.08)
        (name "GND")
        (number "143")
      )
      (pin power_in line (at -5.08 -27.94 0) (length 5.08)
        (name "GND")
        (number "144")
      )
      (pin power_in line (at -5.08 -30.48 0) (length 5.08)
        (name "GND")
        (number "145")
      )
      (pin power_in line (at -5.08 -33.02 0) (length 5.08)
        (name "GND")
        (number "146")
      )
      (pin power_in line (at 50.8 -12.7 180) (length 5.08)
        (name "+5V0_IN")
        (number "15")
      )
      (pin power_in line (at -5.08 -35.56 0) (length 5.08)
        (name "GND")
        (number "155")
      )
      (pin power_in line (at -5.08 -38.1 0) (length 5.08)
        (name "GND")
        (number "156")
      )
      (pin power_in line (at 50.8 -7.62 180) (length 5.08)
        (name "USB0_VBUS")
        (number "16")
      )
      (pin power_in line (at -5.08 -40.64 0) (length 5.08)
        (name "GND")
        (number "168")
      )
      (pin power_in line (at 50.8 -5.08 180) (length 5.08)
        (name "BAT_VDDO")
        (number "17")
      )
      (pin power_out line (at 50.8 -2.54 180) (length 5.08)
        (name "IPS_OUT")
        (number "18")
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "GND")
        (number "33")
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "GND")
        (number "60")
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "GND")
        (number "93")
      )
      (pin input line (at 50.8 -20.32 180) (length 5.08)
        (name "JTAG_TRSTn")
        (number "TP1")
      )
      (pin output line (at 50.8 -43.18 180) (length 5.08)
        (name "X32K0")
        (number "TP10")
      )
      (pin output line (at 50.8 -45.72 180) (length 5.08)
        (name "BOOT0")
        (number "TP11")
      )
      (pin output line (at 50.8 -48.26 180) (length 5.08)
        (name "BOOT1")
        (number "TP12")
      )
      (pin output line (at 50.8 -50.8 180) (length 5.08)
        (name "BOOT2")
        (number "TP13")
      )
      (pin input line (at 50.8 -22.86 180) (length 5.08)
        (name "JTAG_TMS")
        (number "TP2")
      )
      (pin output line (at 50.8 -25.4 180) (length 5.08)
        (name "JTAG_TDO")
        (number "TP3")
      )
      (pin input line (at 50.8 -27.94 180) (length 5.08)
        (name "JTAG_TDI")
        (number "TP4")
      )
      (pin input line (at 50.8 -30.48 180) (length 5.08)
        (name "JTAG_TCK")
        (number "TP5")
      )
      (pin output line (at 50.8 -33.02 180) (length 5.08)
        (name "JMODE0")
        (number "TP6")
      )
      (pin bidirectional line (at 50.8 -35.56 180) (length 5.08)
        (name "JMODE1")
        (number "TP7")
      )
      (pin output line (at 50.8 -38.1 180) (length 5.08)
        (name "TEST_MODE")
        (number "TP8")
      )
      (pin output line (at 50.8 -40.64 180) (length 5.08)
        (name "X24M0")
        (number "TP9")
      )
    )
  )
  (symbol "RanetkaPC_Module_with_PogoPins" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 7.62 2.54 0))
    (property "Value" "RanetkaPC_Module_with_PogoPins" (id 1) (at 17.78 2.54 0))
    (property "Footprint" "RanetkaPC_Module:RanetkaPC_Module_PogoPin" (id 2) (at 20.32 -215.9 0))
    (property "Datasheet" "" (id 3) (at 7.62 2.54 0))
    (property "Mfr. Part Number" "RanetkaPC_Module_V1" (id 4) (at 38.1 -215.9 0))
    (property "ki_locked" "" (id 5) (at 0 0 0))
    (symbol "RanetkaPC_Module_with_PogoPins_1_1"
      (pin input line (at -5.08 -43.18 0) (length 5.08)
        (name "MIPI_CSI_RX_CLK_P")
        (number "1")
      )
      (pin input line (at -5.08 -63.5 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA0_P")
        (number "10")
      )
      (pin input line (at 50.8 -154.94 180) (length 5.08)
        (name "LRADC0")
        (number "100")
      )
      (pin input line (at 50.8 -157.48 180) (length 5.08)
        (name "LRADC1")
        (number "101")
      )
      (pin output line (at 50.8 -144.78 180) (length 5.08)
        (name "HPCOM")
        (number "102")
      )
      (pin output line (at 50.8 -147.32 180) (length 5.08)
        (name "HPR_OUT")
        (number "103")
      )
      (pin output line (at 50.8 -149.86 180) (length 5.08)
        (name "HPL_OUT")
        (number "104")
      )
      (pin bidirectional line (at 50.8 -127 180) (length 5.08)
        (name "UDM1_N")
        (number "105")
      )
      (pin bidirectional line (at 50.8 -129.54 180) (length 5.08)
        (name "UDP1_P")
        (number "106")
      )
      (pin bidirectional line (at 50.8 -162.56 180) (length 5.08)
        (name "CAN0_TX")
        (number "107")
      )
      (pin bidirectional line (at 50.8 -165.1 180) (length 5.08)
        (name "CAN0_RX")
        (number "108")
      )
      (pin bidirectional line (at 50.8 -121.92 180) (length 5.08)
        (name "UDM0_N")
        (number "109")
      )
      (pin input line (at 50.8 -76.2 180) (length 5.08)
        (name "LCD_PWM")
        (number "11")
      )
      (pin bidirectional line (at 50.8 -124.46 180) (length 5.08)
        (name "UDP0_P")
        (number "110")
      )
      (pin bidirectional line (at -5.08 -68.58 0) (length 5.08)
        (name "SDCO_D0")
        (number "111")
      )
      (pin bidirectional line (at -5.08 -71.12 0) (length 5.08)
        (name "SDCO_D1")
        (number "112")
      )
      (pin bidirectional line (at -5.08 -73.66 0) (length 5.08)
        (name "SDCO_D2")
        (number "113")
      )
      (pin bidirectional line (at -5.08 -76.2 0) (length 5.08)
        (name "SDCO_D3")
        (number "114")
      )
      (pin input line (at -5.08 -78.74 0) (length 5.08)
        (name "SDCO_CMD")
        (number "115")
      )
      (pin output line (at -5.08 -81.28 0) (length 5.08)
        (name "SDCO_CLK")
        (number "116")
      )
      (pin input line (at -5.08 -83.82 0) (length 5.08)
        (name "SDC0_DET")
        (number "117")
      )
      (pin output line (at -5.08 -35.56 0) (length 5.08)
        (name "MIPI_CSI_CLK")
        (number "118")
      )
      (pin output line (at -5.08 -38.1 0) (length 5.08)
        (name "MIPI_CSI_FSYNC")
        (number "119")
      )
      (pin input line (at -5.08 -88.9 0) (length 5.08)
        (name "UART2_RX")
        (number "12")
      )
      (pin output line (at 50.8 -208.28 180) (length 5.08)
        (name "EXTEN")
        (number "122")
      )
      (pin output line (at -5.08 -198.12 0) (length 5.08)
        (name "PCI0_PERSTN")
        (number "123")
      )
      (pin input line (at 50.8 -175.26 180) (length 5.08)
        (name "USB0_EN_OCN")
        (number "124")
      )
      (pin input line (at -5.08 -200.66 0) (length 5.08)
        (name "PCI0_WAKE")
        (number "125")
      )
      (pin input line (at -5.08 -203.2 0) (length 5.08)
        (name "PCI0_APP")
        (number "126")
      )
      (pin input line (at -5.08 -195.58 0) (length 5.08)
        (name "PCI0_CLKREQ")
        (number "127")
      )
      (pin no_connect line (at -5.08 -205.74 0) (length 5.08)
        (name "NC")
        (number "128")
      )
      (pin output line (at -5.08 -182.88 0) (length 5.08)
        (name "PCI0_TX0P")
        (number "129")
      )
      (pin output line (at -5.08 -91.44 0) (length 5.08)
        (name "UART2_TX")
        (number "13")
      )
      (pin output line (at -5.08 -180.34 0) (length 5.08)
        (name "PCI0_TX0N")
        (number "130")
      )
      (pin output line (at -5.08 -187.96 0) (length 5.08)
        (name "PCI0_TX1P")
        (number "132")
      )
      (pin output line (at -5.08 -185.42 0) (length 5.08)
        (name "PCI0_TX1N")
        (number "133")
      )
      (pin input line (at -5.08 -177.8 0) (length 5.08)
        (name "PCI0_RX1P")
        (number "135")
      )
      (pin input line (at -5.08 -175.26 0) (length 5.08)
        (name "PCI0_RX1N")
        (number "136")
      )
      (pin input line (at -5.08 -170.18 0) (length 5.08)
        (name "PCI0_RX0N")
        (number "138")
      )
      (pin input line (at -5.08 -172.72 0) (length 5.08)
        (name "PCI0_RX0P")
        (number "139")
      )
      (pin output line (at -5.08 -190.5 0) (length 5.08)
        (name "PCI0_CLKN")
        (number "141")
      )
      (pin output line (at -5.08 -193.04 0) (length 5.08)
        (name "PCI0_CLKP")
        (number "142")
      )
      (pin input line (at 50.8 -195.58 180) (length 5.08)
        (name "JESD_SYNCB_0")
        (number "147")
      )
      (pin input line (at 50.8 -180.34 180) (length 5.08)
        (name "JESD0_CLKX")
        (number "148")
      )
      (pin input line (at 50.8 -182.88 180) (length 5.08)
        (name "JESD0_CKL")
        (number "149")
      )
      (pin output line (at 50.8 -185.42 180) (length 5.08)
        (name "JESD0_SYSREF")
        (number "150")
      )
      (pin output line (at 50.8 -187.96 180) (length 5.08)
        (name "JESD0_SYSREFX")
        (number "151")
      )
      (pin output line (at 50.8 -198.12 180) (length 5.08)
        (name "JESD_SYNCB_0X")
        (number "152")
      )
      (pin input line (at 50.8 -190.5 180) (length 5.08)
        (name "SPARE_LVDS_RX")
        (number "153")
      )
      (pin input line (at 50.8 -193.04 180) (length 5.08)
        (name "SPARE_LVDS_RXX")
        (number "154")
      )
      (pin output line (at 50.8 -111.76 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA2_P")
        (number "157")
      )
      (pin output line (at 50.8 -109.22 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA2_N")
        (number "158")
      )
      (pin output line (at 50.8 -116.84 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA3_P")
        (number "159")
      )
      (pin output line (at 50.8 -114.3 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA3_N")
        (number "160")
      )
      (pin output line (at -5.08 -165.1 0) (length 5.08)
        (name "CLK125")
        (number "161")
      )
      (pin output line (at 50.8 -99.06 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA0_N")
        (number "162")
      )
      (pin output line (at 50.8 -101.6 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA0_P")
        (number "163")
      )
      (pin output line (at 50.8 -106.68 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA1_P")
        (number "164")
      )
      (pin output line (at 50.8 -104.14 180) (length 5.08)
        (name "MIPI_DSI_TX_DATA1_N")
        (number "165")
      )
      (pin output line (at 50.8 -93.98 180) (length 5.08)
        (name "MIPI_DSI_TX_CLK_N")
        (number "166")
      )
      (pin output line (at 50.8 -96.52 180) (length 5.08)
        (name "MIPI_DSI_TX_CLK_P")
        (number "167")
      )
      (pin input line (at 50.8 -205.74 180) (length 5.08)
        (name "PWRGD_RST")
        (number "19")
      )
      (pin input line (at -5.08 -40.64 0) (length 5.08)
        (name "MIPI_CSI_RX_CLK_N")
        (number "2")
      )
      (pin output line (at -5.08 -93.98 0) (length 5.08)
        (name "UART1_TX")
        (number "20")
      )
      (pin input line (at -5.08 -96.52 0) (length 5.08)
        (name "UART1_RX")
        (number "21")
      )
      (pin bidirectional line (at -5.08 -106.68 0) (length 5.08)
        (name "I2C3_SDA/I2C0_SDA")
        (number "22")
      )
      (pin output line (at -5.08 -109.22 0) (length 5.08)
        (name "I2C3_SCK/I2C0_SCK")
        (number "23")
      )
      (pin bidirectional line (at -5.08 -111.76 0) (length 5.08)
        (name "I2C1_SDA")
        (number "24")
      )
      (pin output line (at -5.08 -114.3 0) (length 5.08)
        (name "I2C1_SCK")
        (number "25")
      )
      (pin bidirectional line (at -5.08 -116.84 0) (length 5.08)
        (name "I2C2_SDA")
        (number "26")
      )
      (pin output line (at -5.08 -119.38 0) (length 5.08)
        (name "I2C2_SCK")
        (number "27")
      )
      (pin output line (at -5.08 -99.06 0) (length 5.08)
        (name "UART0_TX")
        (number "28")
      )
      (pin input line (at -5.08 -101.6 0) (length 5.08)
        (name "UART0_RX")
        (number "29")
      )
      (pin input line (at -5.08 -45.72 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA3_P")
        (number "3")
      )
      (pin input line (at 50.8 -170.18 180) (length 5.08)
        (name "USB0_IDDET")
        (number "30")
      )
      (pin input line (at 50.8 -172.72 180) (length 5.08)
        (name "USB0_VBUSDET")
        (number "31")
      )
      (pin bidirectional line (at -5.08 -2.54 0) (length 5.08)
        (name "GPIO1")
        (number "32")
      )
      (pin bidirectional line (at -5.08 -5.08 0) (length 5.08)
        (name "GPIO2")
        (number "34")
      )
      (pin bidirectional line (at -5.08 -7.62 0) (length 5.08)
        (name "GPIO3")
        (number "35")
      )
      (pin bidirectional line (at -5.08 -10.16 0) (length 5.08)
        (name "GPIO4")
        (number "36")
      )
      (pin bidirectional line (at -5.08 -12.7 0) (length 5.08)
        (name "GPIO5")
        (number "37")
      )
      (pin bidirectional line (at -5.08 -15.24 0) (length 5.08)
        (name "GPIO6")
        (number "38")
      )
      (pin bidirectional line (at -5.08 -17.78 0) (length 5.08)
        (name "GPIO7")
        (number "39")
      )
      (pin input line (at -5.08 -48.26 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA3_N")
        (number "4")
      )
      (pin bidirectional line (at -5.08 -20.32 0) (length 5.08)
        (name "GPIO8")
        (number "40")
      )
      (pin bidirectional line (at -5.08 -30.4801 0) (length 5.08)
        (name "GPIO12/RMII0_COL")
        (number "41")
      )
      (pin bidirectional line (at -5.08 -160.02 0) (length 5.08)
        (name "RGMII0_nINT/RMII0_nINT")
        (number "42")
      )
      (pin bidirectional line (at -5.08 -27.94 0) (length 5.08)
        (name "GPIO11/RMII0_CRS")
        (number "43")
      )
      (pin bidirectional line (at -5.08 -157.48 0) (length 5.08)
        (name "RGMII0_TXC/RMII0_TXCLK")
        (number "44")
      )
      (pin bidirectional line (at -5.08 -154.94 0) (length 5.08)
        (name "RGMII0_TXCTL/RMII0_TXEN")
        (number "45")
      )
      (pin bidirectional line (at -5.08 -147.32 0) (length 5.08)
        (name "RGMII0_MDIO/RMII0_MDIO")
        (number "46")
      )
      (pin input line (at -5.08 -144.78 0) (length 5.08)
        (name "RGMII0_MDC/RMII0_MDC")
        (number "47")
      )
      (pin input line (at -5.08 -149.86 0) (length 5.08)
        (name "RGMII0_RXCTL/RMII0_RXDV")
        (number "48")
      )
      (pin output line (at -5.08 -25.4 0) (length 5.08)
        (name "GPIO10/RMII0_RXER")
        (number "49")
      )
      (pin input line (at -5.08 -50.8 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA2_N")
        (number "5")
      )
      (pin input line (at -5.08 -152.4 0) (length 5.08)
        (name "RGMII0_RXC/RMII0_RCLK")
        (number "50")
      )
      (pin output line (at -5.08 -142.24 0) (length 5.08)
        (name "RGMII0_TXD0/RMII0_TXD0")
        (number "51")
      )
      (pin output line (at -5.08 -139.7 0) (length 5.08)
        (name "RGMII0_TXD1/RMII0_TXD1")
        (number "52")
      )
      (pin output line (at -5.08 -137.16 0) (length 5.08)
        (name "RGMII0_TXD2/RMII0_TXD2")
        (number "53")
      )
      (pin output line (at -5.08 -134.62 0) (length 5.08)
        (name "RGMII0_TXD3/RMII0_TXD3")
        (number "54")
      )
      (pin input line (at -5.08 -132.08 0) (length 5.08)
        (name "RGMII0_RXD0/RMII0_RXD0")
        (number "55")
      )
      (pin input line (at -5.08 -129.54 0) (length 5.08)
        (name "RGMII0_RXD1/RMII0_RXD1")
        (number "56")
      )
      (pin input line (at -5.08 -127 0) (length 5.08)
        (name "RGMII0_RXD2/RMII0_RXD2")
        (number "57")
      )
      (pin input line (at -5.08 -124.46 0) (length 5.08)
        (name "RGMII0_RXD3/RMII0_RXD3")
        (number "58")
      )
      (pin output line (at -5.08 -162.56 0) (length 5.08)
        (name "RGMII0_nRST/RMII0_nRST")
        (number "59")
      )
      (pin input line (at -5.08 -53.34 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA2_P")
        (number "6")
      )
      (pin power_out line (at 50.8 -203.2 180) (length 5.08)
        (name "+3V3_IOVCC")
        (number "61")
      )
      (pin input line (at 50.8 -73.66 180) (length 5.08)
        (name "TCP_INT")
        (number "62")
      )
      (pin input line (at 50.8 -71.12 180) (length 5.08)
        (name "LCD_DE")
        (number "63")
      )
      (pin input line (at 50.8 -68.58 180) (length 5.08)
        (name "LCD_VSYNC")
        (number "64")
      )
      (pin input line (at 50.8 -66.04 180) (length 5.08)
        (name "LCD_HSYNC")
        (number "65")
      )
      (pin input line (at 50.8 -63.5 180) (length 5.08)
        (name "LCD_CLK")
        (number "66")
      )
      (pin input line (at 50.8 -60.96 180) (length 5.08)
        (name "LCD_D23")
        (number "67")
      )
      (pin input line (at 50.8 -58.42 180) (length 5.08)
        (name "LCD_D22")
        (number "68")
      )
      (pin input line (at 50.8 -55.88 180) (length 5.08)
        (name "LCD_D21")
        (number "69")
      )
      (pin input line (at -5.08 -55.88 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA1_P")
        (number "7")
      )
      (pin input line (at 50.8 -53.34 180) (length 5.08)
        (name "LCD_D20")
        (number "70")
      )
      (pin input line (at 50.8 -50.8 180) (length 5.08)
        (name "LCD_D19")
        (number "71")
      )
      (pin input line (at 50.8 -48.26 180) (length 5.08)
        (name "LCD_D18")
        (number "72")
      )
      (pin input line (at 50.8 -45.72 180) (length 5.08)
        (name "LCD_D17")
        (number "73")
      )
      (pin input line (at 50.8 -43.18 180) (length 5.08)
        (name "LCD_D16")
        (number "74")
      )
      (pin input line (at 50.8 -40.64 180) (length 5.08)
        (name "LCD_D15")
        (number "75")
      )
      (pin input line (at 50.8 -38.1 180) (length 5.08)
        (name "LCD_D14")
        (number "76")
      )
      (pin input line (at 50.8 -35.56 180) (length 5.08)
        (name "LCD_D13")
        (number "77")
      )
      (pin input line (at 50.8 -33.02 180) (length 5.08)
        (name "LCD_D12")
        (number "78")
      )
      (pin input line (at 50.8 -30.48 180) (length 5.08)
        (name "LCD_D11")
        (number "79")
      )
      (pin input line (at -5.08 -58.42 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA1_N")
        (number "8")
      )
      (pin input line (at 50.8 -27.94 180) (length 5.08)
        (name "LCD_D10")
        (number "80")
      )
      (pin input line (at 50.8 -25.4 180) (length 5.08)
        (name "LCD_D9")
        (number "81")
      )
      (pin input line (at 50.8 -22.86 180) (length 5.08)
        (name "LCD_D8")
        (number "82")
      )
      (pin input line (at 50.8 -20.32 180) (length 5.08)
        (name "LCD_D7")
        (number "83")
      )
      (pin input line (at 50.8 -17.78 180) (length 5.08)
        (name "LCD_D6")
        (number "84")
      )
      (pin input line (at 50.8 -15.24 180) (length 5.08)
        (name "LCD_D5")
        (number "85")
      )
      (pin input line (at 50.8 -12.7 180) (length 5.08)
        (name "LCD_D4")
        (number "86")
      )
      (pin input line (at 50.8 -10.16 180) (length 5.08)
        (name "LCD_D3")
        (number "87")
      )
      (pin input line (at 50.8 -7.62 180) (length 5.08)
        (name "LCD_D2")
        (number "88")
      )
      (pin input line (at 50.8 -5.08 180) (length 5.08)
        (name "LCD_D1")
        (number "89")
      )
      (pin input line (at -5.08 -60.96 0) (length 5.08)
        (name "MIPI_CSI_RX_DATA0_N")
        (number "9")
      )
      (pin input line (at 50.8 -2.54 180) (length 5.08)
        (name "LCD_D0")
        (number "90")
      )
      (pin bidirectional line (at -5.08 -22.86 0) (length 5.08)
        (name "GPIO9")
        (number "91")
      )
      (pin input line (at 50.8 -86.36 180) (length 5.08)
        (name "TPX2")
        (number "92")
      )
      (pin input line (at 50.8 -81.28 180) (length 5.08)
        (name "TPX1")
        (number "94")
      )
      (pin input line (at 50.8 -88.9 180) (length 5.08)
        (name "TPY2")
        (number "95")
      )
      (pin input line (at 50.8 -83.82 180) (length 5.08)
        (name "TPY1")
        (number "96")
      )
      (pin input line (at 50.8 -137.16 180) (length 5.08)
        (name "MIC1_IN")
        (number "97")
      )
      (pin input line (at 50.8 -139.7 180) (length 5.08)
        (name "MIC2_IN")
        (number "98")
      )
      (pin output line (at 50.8 -134.62 180) (length 5.08)
        (name "VMIC")
        (number "99")
      )
    )
    (symbol "RanetkaPC_Module_with_PogoPins_2_1"
      (pin power_in line (at -5.08 -10.16 0) (length 5.08)
        (name "GND")
        (number "120")
      )
      (pin power_in line (at -5.08 -12.7 0) (length 5.08)
        (name "GND")
        (number "121")
      )
      (pin power_in line (at -5.08 -15.24 0) (length 5.08)
        (name "GND")
        (number "131")
      )
      (pin power_in line (at -5.08 -17.78 0) (length 5.08)
        (name "GND")
        (number "134")
      )
      (pin power_in line (at -5.08 -20.32 0) (length 5.08)
        (name "GND")
        (number "137")
      )
      (pin power_in line (at 50.8 -15.24 180) (length 5.08)
        (name "+5V0_IN")
        (number "14")
      )
      (pin power_in line (at -5.08 -22.86 0) (length 5.08)
        (name "GND")
        (number "140")
      )
      (pin power_in line (at -5.08 -25.4 0) (length 5.08)
        (name "GND")
        (number "143")
      )
      (pin power_in line (at -5.08 -27.94 0) (length 5.08)
        (name "GND")
        (number "144")
      )
      (pin power_in line (at -5.08 -30.48 0) (length 5.08)
        (name "GND")
        (number "145")
      )
      (pin power_in line (at -5.08 -33.02 0) (length 5.08)
        (name "GND")
        (number "146")
      )
      (pin power_in line (at 50.8 -12.7 180) (length 5.08)
        (name "+5V0_IN")
        (number "15")
      )
      (pin power_in line (at -5.08 -35.56 0) (length 5.08)
        (name "GND")
        (number "155")
      )
      (pin power_in line (at -5.08 -38.1 0) (length 5.08)
        (name "GND")
        (number "156")
      )
      (pin power_in line (at 50.8 -7.62 180) (length 5.08)
        (name "USB0_VBUS")
        (number "16")
      )
      (pin power_in line (at -5.08 -40.64 0) (length 5.08)
        (name "GND")
        (number "168")
      )
      (pin power_in line (at 50.8 -5.08 180) (length 5.08)
        (name "BAT_VDDO")
        (number "17")
      )
      (pin power_out line (at 50.8 -2.54 180) (length 5.08)
        (name "IPS_OUT")
        (number "18")
      )
      (pin power_in line (at -5.08 -2.54 0) (length 5.08)
        (name "GND")
        (number "33")
      )
      (pin power_in line (at -5.08 -5.08 0) (length 5.08)
        (name "GND")
        (number "60")
      )
      (pin power_in line (at -5.08 -7.62 0) (length 5.08)
        (name "GND")
        (number "93")
      )
      (pin input line (at 50.8 -20.32 180) (length 5.08)
        (name "JTAG_TRSTn")
        (number "TP1")
      )
      (pin output line (at 50.8 -43.18 180) (length 5.08)
        (name "X32K0")
        (number "TP10")
      )
      (pin output line (at 50.8 -45.72 180) (length 5.08)
        (name "BOOT0")
        (number "TP11")
      )
      (pin output line (at 50.8 -48.26 180) (length 5.08)
        (name "BOOT1")
        (number "TP12")
      )
      (pin output line (at 50.8 -50.8 180) (length 5.08)
        (name "BOOT2")
        (number "TP13")
      )
      (pin input line (at 50.8 -22.86 180) (length 5.08)
        (name "JTAG_TMS")
        (number "TP2")
      )
      (pin output line (at 50.8 -25.4 180) (length 5.08)
        (name "JTAG_TDO")
        (number "TP3")
      )
      (pin input line (at 50.8 -27.94 180) (length 5.08)
        (name "JTAG_TDI")
        (number "TP4")
      )
      (pin input line (at 50.8 -30.48 180) (length 5.08)
        (name "JTAG_TCK")
        (number "TP5")
      )
      (pin output line (at 50.8 -33.02 180) (length 5.08)
        (name "JMODE0")
        (number "TP6")
      )
      (pin bidirectional line (at 50.8 -35.56 180) (length 5.08)
        (name "JMODE1")
        (number "TP7")
      )
      (pin output line (at 50.8 -38.1 180) (length 5.08)
        (name "TEST_MODE")
        (number "TP8")
      )
      (pin output line (at 50.8 -40.64 180) (length 5.08)
        (name "X24M0")
        (number "TP9")
      )
    )
  )
)
