(footprint "RanetkaPC_Module_PogoPin" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6277F468)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 30.5) (layer "F.SilkS"))
  (fp_text value "RanetkaPC_Module_PogoPin" (at 1 32) (layer "F.Fab"))
  (fp_text user "* RanetkaPC ver 1.3" (at 0 -9 unlocked) (layer "F.SilkS"))
  (fp_text user "Supported SOM modules:" (at 0.5 -17.5 unlocked) (layer "F.SilkS"))
  (fp_text user "(C) Fabmicro, LLC., Tyumen, Russia." (at 0 1.5 unlocked) (layer "F.SilkS"))
  (fp_text user "${ISSUE_DATE}" (at -0.055522 4.5 unlocked) (layer "F.SilkS"))
  (fp_text user "* Module_A20 ver 1.3" (at 0.5 -13 unlocked) (layer "F.SilkS"))
  (fp_text user "SOM module development kit and test jig" (at 0 -21.5 unlocked) (layer "F.SilkS"))
  (pad "1" thru_hole oval (at -31 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at -29 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at -27 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at -25 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "5" thru_hole oval (at -23 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "6" thru_hole oval (at -21 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "7" thru_hole oval (at -19 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "8" thru_hole oval (at -17 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "9" thru_hole oval (at -15 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "10" thru_hole oval (at -13 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "11" thru_hole oval (at -11 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "12" thru_hole oval (at -9 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -7 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "14" thru_hole oval (at -5 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "15" thru_hole oval (at -3 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "16" thru_hole oval (at -1 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "17" thru_hole oval (at 1 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "18" thru_hole oval (at 3 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "19" thru_hole oval (at 5 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "20" thru_hole oval (at 7 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "21" thru_hole oval (at 9 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "22" thru_hole oval (at 11 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "23" thru_hole oval (at 13 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "24" thru_hole oval (at 15 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "25" thru_hole oval (at 17 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "26" thru_hole oval (at 19 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "27" thru_hole oval (at 21 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "28" thru_hole oval (at 23 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "29" thru_hole oval (at 25 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "30" thru_hole oval (at 27 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "31" thru_hole oval (at 29 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "32" thru_hole oval (at 31 26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "33" thru_hole oval (at 33 27) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "34" thru_hole oval (at 33 25) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "35" thru_hole oval (at 33 23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "36" thru_hole oval (at 33 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "37" thru_hole oval (at 33 19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "38" thru_hole oval (at 33 17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "39" thru_hole oval (at 33 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "40" thru_hole oval (at 33 13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "41" thru_hole oval (at 33 11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "42" thru_hole oval (at 33 9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "43" thru_hole oval (at 33 7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "44" thru_hole oval (at 33 5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "45" thru_hole oval (at 33 3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "46" thru_hole oval (at 33 1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "47" thru_hole oval (at 33 -1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "48" thru_hole oval (at 33 -3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "49" thru_hole oval (at 33 -5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "50" thru_hole oval (at 33 -7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "51" thru_hole oval (at 33 -9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "52" thru_hole oval (at 33 -11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "53" thru_hole oval (at 33 -13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "54" thru_hole oval (at 33 -15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "55" thru_hole oval (at 33 -17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "56" thru_hole oval (at 33 -19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "57" thru_hole oval (at 33 -21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "58" thru_hole oval (at 33 -23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "59" thru_hole oval (at 33 -25) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "60" thru_hole oval (at 33 -27) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "61" thru_hole oval (at 31 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "62" thru_hole oval (at 29 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "63" thru_hole oval (at 27 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "64" thru_hole oval (at 25 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "65" thru_hole oval (at 23 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "66" thru_hole oval (at 21 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "67" thru_hole oval (at 19 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "68" thru_hole oval (at 17 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "69" thru_hole oval (at 15 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "70" thru_hole oval (at 13 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "71" thru_hole oval (at 11 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "72" thru_hole oval (at 9 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "73" thru_hole oval (at 7 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "74" thru_hole oval (at 5 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "75" thru_hole oval (at 3 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "76" thru_hole oval (at 1 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "77" thru_hole oval (at -1 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "78" thru_hole oval (at -3 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "79" thru_hole oval (at -5 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "80" thru_hole oval (at -7 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "81" thru_hole oval (at -9 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "82" thru_hole oval (at -11 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "83" thru_hole oval (at -13 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "84" thru_hole oval (at -15 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "85" thru_hole oval (at -17 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "86" thru_hole oval (at -19 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "87" thru_hole oval (at -21 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "88" thru_hole oval (at -23 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "89" thru_hole oval (at -25 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "90" thru_hole oval (at -27 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "91" thru_hole oval (at -29 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "92" thru_hole oval (at -31 -26 270) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "93" thru_hole oval (at -33 -27) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "94" thru_hole oval (at -33 -25) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "95" thru_hole oval (at -33 -23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "96" thru_hole oval (at -33 -21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "97" thru_hole oval (at -33 -19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "98" thru_hole oval (at -33 -17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "99" thru_hole oval (at -33 -15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "100" thru_hole oval (at -33 -13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "101" thru_hole oval (at -33 -11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "102" thru_hole oval (at -33 -9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "103" thru_hole oval (at -33 -7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "104" thru_hole oval (at -33 -5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "105" thru_hole oval (at -33 -3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "106" thru_hole oval (at -33 -1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "107" thru_hole oval (at -33 1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "108" thru_hole oval (at -33 3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "109" thru_hole oval (at -33 5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "110" thru_hole oval (at -33 7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "111" thru_hole oval (at -33 9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "112" thru_hole oval (at -33 11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "113" thru_hole oval (at -33 13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "114" thru_hole oval (at -33 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "115" thru_hole oval (at -33 17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "116" thru_hole oval (at -33 19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "117" thru_hole oval (at -33 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "118" thru_hole oval (at -33 23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "119" thru_hole oval (at -33 25) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "120" thru_hole oval (at -33 27) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "121" thru_hole oval (at -31 23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "122" thru_hole oval (at -31 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "123" thru_hole oval (at -31 19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "124" thru_hole oval (at -31 17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "125" thru_hole oval (at -31 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "126" thru_hole oval (at -31 13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "127" thru_hole oval (at -31 11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "128" thru_hole oval (at -31 9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "129" thru_hole oval (at -31 7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "130" thru_hole oval (at -31 5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "131" thru_hole oval (at -31 3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "132" thru_hole oval (at -31 1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "133" thru_hole oval (at -31 -1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "134" thru_hole oval (at -31 -3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "135" thru_hole oval (at -31 -5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "136" thru_hole oval (at -31 -7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "137" thru_hole oval (at -31 -9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "138" thru_hole oval (at -31 -11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "139" thru_hole oval (at -31 -13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "140" thru_hole oval (at -31 -15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "141" thru_hole oval (at -31 -17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "142" thru_hole oval (at -31 -19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "143" thru_hole oval (at -31 -21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "144" thru_hole oval (at -31 -23) (size 1.87 1.7) (drill 1.4) (layers *.Cu *.Mask))
  (pad "145" thru_hole oval (at 31 -23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "146" thru_hole oval (at 31 -21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "147" thru_hole oval (at 31 -19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "148" thru_hole oval (at 31 -17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "149" thru_hole oval (at 31 -15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "150" thru_hole oval (at 31 -13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "151" thru_hole oval (at 31 -11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "152" thru_hole oval (at 31 -9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "153" thru_hole oval (at 31 -7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "154" thru_hole oval (at 31 -5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "155" thru_hole oval (at 31 -3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "156" thru_hole oval (at 31 -1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "157" thru_hole oval (at 31 1) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "158" thru_hole oval (at 31 3) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "159" thru_hole oval (at 31 5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "160" thru_hole oval (at 31 7) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "161" thru_hole oval (at 31 9) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "162" thru_hole oval (at 31 11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "163" thru_hole oval (at 31 13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "164" thru_hole oval (at 31 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "165" thru_hole oval (at 31 17) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "166" thru_hole oval (at 31 19) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "167" thru_hole oval (at 31 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "168" thru_hole oval (at 31 23) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP1" thru_hole oval (at 22.5 18.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP2" thru_hole oval (at 22.5 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP3" thru_hole oval (at 17.5 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP4" thru_hole oval (at 20 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP5" thru_hole oval (at 20 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP6" thru_hole oval (at 12 17.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP7" thru_hole oval (at 9.5 17.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP8" thru_hole oval (at 15 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP9" thru_hole oval (at 2.5 13) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP10" thru_hole oval (at 2.5 15.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP11" thru_hole oval (at -4 12.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP12" thru_hole oval (at -4 15) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP13" thru_hole oval (at -4 17.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP14" thru_hole oval (at -12 18.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP15" thru_hole oval (at -12 11) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP16" thru_hole oval (at -12 16) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP17" thru_hole oval (at -12 13.5) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
  (pad "TP18" thru_hole oval (at -12 21) (size 1.87 1.70) (drill 1.4) (layers *.Cu *.Mask))
)
